

SECTION 10 31 00

MANUFACTURED GAS FIREPLACES

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

PART 1 GENERAL

1.1 SECTION INCLUDES

A. Gas fireplaces and accessories including the following:

 1. Manufactured indoor gas fireplaces.

 2. Manufactured indoor/outdoor gas fireplaces

 3. Manufactured outdoor gas fireplaces.

 4. Gas fireplace accessories.

1.2 RELATED SECTIONS

A. Section 06 10 00 - Rough Carpentry.

B. Section 22 14 13 - Facility Storm Drainage Piping.

C. Section 26 05 00 - Common Work Results for Electrical.

1.3 REFERENCES

A. ANSI Z21.44 - Gas-Fired Gravity and Fan Type Direct Vent Wall Furnaces.

B. ANSI Z21.88 - Vented Gas Fireplace Heaters.

C. Z21.50b - Vented Gas Fireplaces.

D. ANSI Z223.1 - National Fuel Gas Code.

E. CSA 2.22b - Vented Gas Fireplaces.

F. CSA 2.33 - Vented Gas Fireplace Heaters.

G. CAN/ULC S610 - Factory-Built Fireplaces.

H. UL 127 - Standard for Factory-Built Fireplaces.

I. UL 907 - Standard for Fireplace Accessories

J. UL 1482 - Standard for Safety for Solid-Fuel Type Room Heaters.

1.4 SUBMITTALS

A. Submit under provisions of Section 01 30 00 - Administrative Requirements.

B. Product Data: Manufacturer's data sheets on each product to be used, including:

 1. Preparation instructions and recommendations.

 2. Storage and handling requirements and recommendations.

 3. Installation methods.

C. Shop Drawings: Provide drawing of required clearances, rough-in of enclosure and utilities.

 1. Selection Samples: For each finish product specified, two complete sets of color chips

 representing manufacturer's full range of available colors and finishes.

D. Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square representing actual product.

1.5 QUALITY ASSURANCE

A. Manufacturer Qualifications: Minimum 5 year experience manufacturing similar products.

B. Installer Qualifications: Minimum 2 year experience installing similar products.

C. Multiple Installation Mock-Up: Provide a mock-up for evaluation of site and framing preparation techniques and installation workmanship.

 1. Provide representative fireplace in area designated by Architect.

 2. Do not proceed with remaining units until workmanship, installation and operation are approved by Architect.

 3. Remake mock-up unit as required to produce acceptable work.

1.6 PRE-INSTALLATION MEETINGS

A. Convene minimum two weeks prior to starting work of this section.

1.7 DELIVERY, STORAGE, AND HANDLING

A. Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.

B. Handling: Handle materials to avoid damage.

1.8 PROJECT CONDITIONS

A. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.

1.9 SEQUENCING

A. Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.

1.10 WARRANTY

A. Warranty: Provide manufacturer's standard warranty against defects in materials and workmanship.

PART 2 PRODUCTS

2.1 MANUFACTURERS

A. Acceptable Manufacturer: Heat & Glo®, which is located at: 7571 215th St. W.; Lakeville, MN 55044; Toll Free Tel: 800-669-HEAT (4328); Email:request info (swansonm@hearthnhome.com); Web:www.heatnglo.com

B. Substitutions: Not permitted.

C. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

2.2 MANUFACTURED WOOD FIREPLACES

A. General:

1. Comply with applicable building codes.

2. Comply with UL 127.

3. Comply with portions of UL 1482 and UL 907 applicable.

**Exclaim Wood Fireplace:**

1. Fronts-Doors: Black Grand Vista.

2. Fronts-Doors: Bronze Grand Vista.

3. Fronts-Doors: Black Contour.

4. Fronts-Doors: Bronze Contour.

5. Fronts-Doors: Black DM Glass Door.

6. Gas Log Set: Grand Oak Gas Logs.

7. Refractory: Traditional.

8. Refractory: Herringbone.

9. Cast Mantels: As specified.

10. Mantel Shelf: As specified.

11. Model Exclaim-36 as manufactured by Heat & Glo.

a. Unit Front Width: 44-1/2 inches (1130 mm).

b. Framing Front Width: 45-1/2 inches (1156 mm).

c. Unit Back Width: 28-5/8 inches 9727 mm).

d. Framing Back Width: 45-1/2 inches (1156 mm).

e. Unit Front Height with standoffs: 59-1/4 inches (1505 mm).

f. Framing Front Height (rough opening): 59-3/4 inches (1518 mm).

g. Unit Rear Height: 59-1/4 inches (1505 mm).

h. Framing Rear Height: 59-3/4 inches (1518 mm).

i. Unit Depth: 27-1/2 inches (699 mm).

j. Framing Depth: 28 inches (711 mm).

k. Firebox Opening: 36 inches x 28-1/2 inches (914 mm x 724 mm).

12. Model EXCLAIM-42 as manufactured by Heat & Glo.

a. Unit Front Width: 50-1/2 inches (1283 mm).

b. Framing Front Width: 51-1/2

c. Unit Back Width: 34-1/2

d. Framing Back Width: 51-1/2

e. Unit Front Height with standoffs: 59-1/4 inches (1505 mm).

f. Framing Front Height (rough opening): 59-3/4 inches (1518 mm).

g. Unit Rear Height: 59-1/4 inches (1505 mm).

h. Framing Rear Height: 59-3/4 inches (1518 mm).

i. Unit Depth: 27-1/2 inches (699 mm).

j. Framing Depth: 28-1/2 inches (724 mm).

k. Firebox Opening: 42 inches x 28-1/2 inches (1067 mm x 724 mm).

13. Model Exclaim-50 as manufactured by Heat & Glo.

a. Unit Front Width: 60-5/8 inches (1546 mm).

b. Framing Front Width: 61-5/8 inches (1565 mm).

c. Unit Back Width: 41-5/8 inches (1057 mm).

d. Framing Back Width: 61-5/8 inches (1565 mm).

e. Unit Front Height with standoffs: 70-1/2 inches (1791 mm).

f. Framing Front Height (rough opening): 71 inches (1803 mm).

g. Unit Rear Height: 70-1/2 inches (1791 mm).

h. Framing Rear Height: 71 inches (1803 mm).

i. Unit Depth: 29-1/2 inches (749 mm).

j. Framing Depth: 30-1/2 inches (775 mm).

k. Firebox Opening: 50 inches x 33 inches (1270 mm x 838 mm).